A VCP driver is required for the SEANEXX USB AIS receiver.
It will be installed automatically, during installation of SEANEXX Connect.
Be aware to install SEANEXX Connect (incl. the VCP driver) prior connecting the SEANEXX USB receiver to your PC/notebook
for the first time.